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DEPARTMENT:  INFORMATION COMMUNICATION TECHNOLOGY
SUMMATIVE OBSERVATION CHECKLIST — VARIANT A
	Candidate's Name & Registration Code
	

	Assessor's Name & Registration Code
	

	Venue of Assessment
	

	Date of Assessment
	

	Items to be Evaluated: Please award marks as appropriate, tick the competence reached and give a brief comment on your observation.
	Marks Available
	Marks Obtained
	Competent / Not Yet Competent
	Comments

	TASK 1: Terminate and certify the horizontal cabling:

	[PC 1.5]  Selected serviceable tools and the correct cable and connectors for the specification.
Marking points: Crimper, stripper, punch-down tool and tester selected and checked; Cat 6 cable and Cat 6 connectors used.
	5
	
	C  ☐    NYC  ☐
	

	[PC 2.4]  Routed and dressed the runs within bend radius and trunking fill limits.
Marking points: No kink or sharp bend; trunking not overfilled; service loop at each end; data separated from power.
	8
	
	C  ☐    NYC  ☐
	

	[PC 1.7]  Stripped sheath to the specified length without damaging the conductors.
Marking points: 12–13 mm strip on every termination; no nicked insulation.
	6
	
	C  ☐    NYC  ☐
	

	[PC 1.8]  Arranged conductors in the declared scheme with untwist within limits.
Marking points: T568B at every point; untwist under 13 mm; sequence correct on all six terminations.
	8
	
	C  ☐    NYC  ☐
	

	[PC 2.3]  Punched down the outlets and patch panel ports correctly.
Marking points: Conductors fully seated by the tool; excess trimmed flush; no conductor left proud of the IDC.
	6
	
	C  ☐    NYC  ☐
	

	[PC 1.11]  Certified or tested every run and cord and recorded the results.
Marking points: Wire map read and recorded for all runs and cords; failures re-terminated and re-tested; schedule complete and legible.
	7
	
	C  ☐    NYC  ☐
	

	Subtotal 1
	40
	
	
	

	TASK 2: Connect and configure the network:

	[PC 2.2]  Mounted the devices in the cabinet with correct positioning and airflow.
Marking points: Panel above or below its switch; fixings secure; airflow unobstructed; power leads clear of data cords.
	6
	
	C  ☐    NYC  ☐
	

	[PC 2.5]  Interconnected the devices to form the specified topology.
Marking points: Workstations to switch, switch uplink to router; star topology correctly formed and explained.
	8
	
	C  ☐    NYC  ☐
	

	[PC 2.6]  Produced and applied a correct IP addressing scheme.
Marking points: Addresses within 192.168.50.0/24, no duplicates, correct mask and gateway on every device; plan documented before configuring.
	8
	
	C  ☐    NYC  ☐
	

	[PC 2.1]  Observed safety measures and PPE throughout the task.
Marking points: PPE worn; power isolated before cabinet work; no trip hazards left in the walkway.
	5
	
	C  ☐    NYC  ☐
	

	[PC 2.7]  Verified connectivity across the network and recorded each result.
Marking points: Ping to peer, switch, gateway and external host all demonstrated and recorded; link speed confirmed.
	8
	
	C  ☐    NYC  ☐
	

	Subtotal 2
	35
	
	
	

	TASK 3: Diagnose, repair and document a fault:

	[PC 3.1]  Selected appropriate monitoring or test tools for the symptom presented.
Marking points: Tool choice matches the layer being investigated — tester for cabling, ipconfig/ping for addressing, switch statistics for port errors.
	4
	
	C  ☐    NYC  ☐
	

	[PC 3.2]  Monitored the network and interpreted the indicators correctly.
Marking points: Link lights, port statistics or ping results read and correctly interpreted to the assessor.
	5
	
	C  ☐    NYC  ☐
	

	[PC 3.3]  Followed a structured diagnostic procedure and localised the fault.
Marking points: Worked outward from the symptom in a logical order; substitution used to isolate; the fault correctly identified with supporting evidence.
	7
	
	C  ☐    NYC  ☐
	

	[PC 3.4]  Repaired or replaced the faulty component and proved the network restored.
Marking points: Repair carried out safely and correctly; connectivity re-tested and demonstrated to the assessor.
	6
	
	C  ☐    NYC  ☐
	

	[PC 3.5]  Completed a maintenance log entry to workplace standard.
Marking points: Date, fault reported, fault found, action taken, verification result and technician name all recorded.
	3
	
	C  ☐    NYC  ☐
	

	Subtotal 3
	25
	
	
	

	GRAND TOTAL
	100
	
	
	



ASSESSMENT OUTCOME
The candidate was found to be:    Competent  ☐    Not Yet Competent  ☐
(The candidate is competent if they obtain at least 50 % overall AND are judged Competent on every performance criterion above.)
Feedback from the Candidate: ____________________________________________________________
Feedback to the Candidate:   ____________________________________________________________
Candidate's Signature: ______________________     Date: ____________
Assessor's Signature:  ______________________     Date: ____________
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